|  |  |
| --- | --- |
| **TRACK LAYING EQUIPMENT** | |
| D:\r&M web\Revised Website\4.maintenance vehicle\track laying vehicle\TRACK LAYING EQPT..jpg | |
|  | |
| Lifting Capacity | 9 Tonne |
| Max. Lift of Rail Clamp | 2,900 mm from Ground Level |
| **Engine** Make / **Model Power** | Kirloskar Oil Engine Limited (KOEL) / HA 694 79 kW (106 hp) ~ 2,300 rpm |
| **Drive System** | Hydraulic Drive Provided by Engine Driven variable Displacement Pump to Wheels through Hydraulic Motor and Chain, forward and reverse Drive Possible |
| Rail Clamps | Panel Lifting done by 4 Independent Scissor Mechanisms Operated by Hydraulic Cylinders· |
| **Sleeper Grippers** | Hydraulically Operated Angle Grippers Provided for Loading and Unloading of Concrete Sleepers |
| **Brakes** | Hydraulically Operated Shoe Brakes on all 4 Wheels Actuated by Hydraulically Operated Valves, Parking Brake on all 4 wheels |
| **Weight of Equipment** | 12,000 kgs |
| Max. Speed | 14 Kmph |
| **Dimensions (in mm)** Length Width | 3,100 (including Bridge) 3,860 |
| Height Track Gauge | 2,560 (Bridge Lowered) 3,400 (Auxiliary Track Gauge) |