**ANNEXURE-I**

**E-TENDER BID INVITATION NO.6300028861**

**COMPLIANCE TO TECHNICAL SPECIFICATIONS**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S.No** | **Material** | **Detailed Text** | **Tender Qty** | **Unit** | **COMPILED / NOT COMPILED TO SPECIFICATION MENTIONED IN THE DESCRIPTION** | **REMARKS** |
| 1 | RFN2950664 | HEX NUT -M6,PC-5,GALVANISED | 2,925 | Nos |  |  |
| 2 | RFN3811211 | HEX. HD. NUT M12, TO IS:1364-Part 3, PC-6,COARSE PITCH GLVD (HDZ OF IS: 4759-96) | 11,350 | Nos |  |  |
| 3 | RFN5431016 | NUT PREVALING TORQUE M10 TO SPECFICATION IS:7002-91, PC- 8, WITH NICKLE PLATING. | 2,700 | Nos |  |  |
| 4 | RFN5431624 | HEX. NUT PREVAILING TARQUE TYPE-M16 TO IS:7002-91, PC-8 WITH NICKEL PLATING. | 725 | Nos |  |  |
| 5 | RFS3631025 | HEX. HEAD SCREW M10 X 25 LONG. TO IS: 1363 (Pt-2)-2002 / IS:1367(P-14)-8 4, Gr-A2-70 | 14,710 | Nos |  |  |
| 6 | RPS2530819 | SLTD PAN HD TAPP SCREW ST4.2X19 | 2,700 | Nos |  |  |
| 7 | RFR0330512 | FLAT CSK HEAD 90° RIVET DIA 5 X 12 TO IS: 2907-98, TABLE-2, ALUMINIUM , COATING TO AC25 | 3,100 | Nos |  |  |
| 8 | RFR0330520 | FLAT CSK HEAD 90° RIVET DIA 5 X 20 TO IS: 2907-98, TABLE-2, ALUMINIUM , COATING TO AC25 | 2,900 | Nos |  |  |
| 9 | RFR0840312 | SNAP HEAD NON FERROUS RIVET DIA 3 X12, IS: 2907-98, TABLE-1 /MATL: IS:74 0-77, Gr-64430 | 22,500 | Nos |  |  |
| 10 | CFN0110652 | HEX NUT M6 TO STD CFN01 | 47343 | Nos |  |  |
| 11 | CFN0120652 | "NUT, HEX. M6 TO BEML STD.CFN01" | 122278 | Nos |  |  |
| 12 | RFN3322564 | "NUT, LOCK DIA 25 TO IS:3837-76, TABLE-6, ALUMINIUM TO IS:733" GR.63400WP | 17235 | Nos |  |  |
| 13 | CFS0110820 | HEX HEAD SCREW M8X20 TO COMPANY STD. NO. CFS 01 10820. | 150 | Nos |  |  |
| 14 | CFS0120620 | SCREW HEX HD M6X20 -1C.P-GR- 8.8 AS PER STD CFS01. | 8649 | Nos |  |  |
| 15 | CFS0210420 | SCREW, SLOTTED CHEESE HEAD M4X20 TO BEML STD.CFS02 | 1845 | Nos |  |  |
| 16 | CFS0210610 | SCREW, SLOTTED CHEESE HEAD M6X10 TO BEML STD.CFS02 | 99775 | Nos |  |  |
| 17 | CFS0210616 | SCREW, SLOTTED CHEESE HEAD M6X16 TO BEML STD.CFS02 | 115800 | Nos |  |  |
| 18 | RFS2120625 | SLOTTED CSK FLAT HEAD TAPPING SCREW ST 3.5x25-C TO IS: 7170-1989, MATL - IS 1367 (P14)-84, Gr-A2-70 | 27450 | Nos |  |  |
| 19 | RFS5160620 | RFS5160620,HEX. HEAD SCREW, M6 X 20 TO IS 1364 PART 2 2002 MATL IS 1367 P14 Gr A2 70 ISO 3506 79, Gr A2 70, STAINLESS STEEL | 1750 | Nos |  |  |
| 20 | RFS5160812 | STAINLESS STEEL HEX HEAD SCREW M8 X 12 TO IS:1364 (PART.2) T 1. | 10725 | Nos |  |  |
| 21 | RFS5160840 | RFS5160840,HEX. HEAD SCREW, M8 X 40 TO IS 1364 PART 2 2002 MATL IS 1367 P14 Gr A2 70 ISO 3506 79, Gr A2 70, STAINLESS STEEL | 22050 | Nos |  |  |
| 22 | RFS6220425 | CH. HEAD SCREW AM4x25 TO IS 1366-2002, MATL - IS 1367 (P14), Gr-A2-70 | 14625 | Nos |  |  |
| 23 | RFS6220520 | CH. HEAD SCREW AM5x20 TO IS 1366-2002, MATL - IS 1367 (P14), Gr-A2-70 | 675 | Nos |  |  |
| 24 | RFS6220550 | M5X50SSCH.HD.SCREW | 62325 | Nos |  |  |
| 25 | RFS6220620 | CH. HEAD SCREW AM6x20 TO IS 1366-2002, MATL - IS 1367 (P14), Gr-A2-70 | 10947 | Nos |  |  |
| 26 | CFW0110619 | SPRING WASHER M6 TO BEML STD. CFW01 (ZINC PLATING WITH YELLOW CHROMATE PASSIVATION AS PER IS:1573-1986, 15µm THK) | 224475 | Nos |  |  |
| 27 | CFW0110825 | SPRING WASHER M8 TO BEML STD. CFW01 (ZINC PLATING WITH YELLOW CHROMATE PASSIVATION AS PER IS:1573-1986, 15µm THK) | 14750 | Nos |  |  |
| 28 | CFW0210616 | WASHER - PLAIN M6 X 1.6 as per std | 213125 | Nos |  |  |
| 29 | CFW0210816 | AS PER STD. (ZINC PLATING WITH YELLOW CHROMATE PASSIVATION AS PER IS:1573-1986, 15µm THK) | 12950 | Nos |  |  |
| 30 | RFW0910410 | SPRING WASHER - B 4,IS: 3063-94, TYPE-B, STEEL , Zn + Cr | 2025 | Nos |  |  |
| 31 | RFW0920512 | RFW0920512, SPRING WASHER-B5,TO IS:3063-94/ MATL:SS: 1367(P-14)-84, A2- 70.Stainless Steel | 62425 | Nos |  |  |
| 32 | RFW0930616 | SPRING WASHER - B6 TO IS:3063-1994, DACROTIZE TO SPEC ASTM F1136 GR-2, | 15075 | Nos |  |  |
| 33 | RFW0930820 | SPRING WASHER B8 TO IS:3063-1994,DACROTIZE TO SPEC. ASTM F1136 GR-6 WITH BLACK TOP COAT | 35775 | Nos |  |  |
| 34 | RFW0950409 | SPRING WASHER - B 4 TO IS: 3063-94, TYPE-B, STEEL , GLVD | 14625 | Nos |  |  |
| 35 | RFW1730616 | RFW1730616,PUNCHED WASHER FOR M6 BOLT TO IS 2016 TAB 2 1967 MAT L AISI 304 IS 1367 P14 Gr A2 70, STAINLESS STEEL | 20609 | Nos |  |  |
| 36 | RFW1730408 | PUNCHED WASHER A4.5 TO IS 2016-67, TAB 2, MATL - AISI 304 | 12697 | Nos |  |  |
| 37 | RFW1730510 | PUNCHED WASHER FOR M5 BOLT TO IS:2016-(TAB-2)- 1967 / MATL :AISI-304 / IS:1367-(P14)-Gr-A2-70, STAINLESS STEEL | 56825 | Nos |  |  |
| 38 | RFW1730816 | PUNCHED WASHER A9 TO IS:2016-(TAB-2)-1967 / MATL:AISI-304 / IS:1367- (P14)-Gr-A2-70,STAINLESS STEEL | 35775 | Nos |  |  |

|  |  |  |
| --- | --- | --- |
| **Column (A)** | **Column (B)** | **Column (C)**  **(say ‘Yes’ OR ‘’No” in this column, as applicable)** |
| **1** | Confirmation whether the bidding firm is ICF/RCF/BEML/RDSO source. |  |
| **2** | The technical requirement as mentioned in item description above is fully understood by the bidding firm and firm is bidding for the same. |  |
| **3** | **Are you an Manufacturer of Hardware / Authorised dealers of reputed make of hardware.**  Kindly confirm and attach relevant documents |  |
| **3** | \*Confirmation from the bidding firm that it does not have any history of pending litigations and Risk purchase against previous orders of BEML, as bids from such firms are liable for rejection.  **(If ‘YES’ is mentioned in Column 3 it would mean there is no history and if ‘NO’ is mentioned in Column 3 it would mean there is a history)** |  |

NOTE:State ‘**YES’ / ‘NO’** as applicable in column (C).

\*Bids of firms having any history of pending litigations , default in and Risk purchase against previous orders of BEML which mention otherwise in this bid confirmation are liable for rejection.

**Name and Signature of authorised rep.**

**of Bidding firm with Seal**