**ANNEXURE A**

**COMPLIANCE TO TECHNICAL SPECIFICATIONS**

E-TENDER : BR01/RM2/6300030897

ITEM : HARDWARE ITEMS – 17 TYPES

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.No | Material | | Description | Quantity Requested | UOM | Compiled/Not Compiled | Remarks | |
| 1 | RFN0191615 | | RFN0191615,HEX. HEAD NUT M 16, TO IS 1364 PT 3 2002, PC 8, DACROTIZE TO SPEC ASTM F1136 GR 6 WITH BLACK TOP COAT | 792 | NO |  |  | |
| 2 | RFN3860432 | | RFN3860432,HEX. HEAD NUT M4 TO IS 1364 PART 3 2002 MATL ISO 3506 79, Gr A2 70,STAINLESS STEEL | 648 | NO |  |  | |
| 3 | RFN3860868 | | RFN3860868,HEX. HEAD NUT M8 TO IS 1364 PART 3 2002 MATL ISO 3506 79 , Gr A2 70,STAINLESS STEEL | 360 | NO |  |  | |
| 4 | RFN3890868 | | HEX. HEAD NUT M8 (GEOMET SPEC)  HEX NUT,TO IS:1364 (PART-3)-2002, PC-10, GEOMET TO SPEC. ASTM F1136 Gr.-6 WITH BLACK TOP COAT | 360 | NO |  |  | |
| 5 | RFN4091680 | | RFN4091680,HEX. THIN NUT M16 TO IS 1364 PT 4 2003, PC 8, DACROTIZE TO SPEC ASTM F1136 GR 6 WITH BLACK TOP COAT | 792 | NO |  |  | |
| 6 | RFS0171650 | | RFS0171650,HEX. HEAD SCREW, M16 X 50 TO IS 1364 PART 2 2002, PC 8.8, DACROTIZE TO STANDARD ASTM F 1136 04 Grade 6 WITH BLACK TOP COAT | 792 | NO |  |  | |
| 7 | RFS5160416 | | RFS5160416,HEX. HEAD SCREW, M4 X 16 TO IS 1364 PART 2 2002 MATL IS 1367 P14 Gr A2 70 ISO 3506 79, Gr A2 70, STAINLESS STEEL | 648 | NO |  |  | |
| 8 | RFS5160820 | | RFS5160820,HEX. HEAD SCREW, M8X 20 TO IS 1364 PART 2 2002 MATL IS 1367 P14 Gr A2 70 ISO 3506 79, Gr A2 70, STAINLESS STEEL | 1584 | NO |  |  | |
| 9 | RFS5160825 | | RFS5160825,HEX. HEAD SCREW, M8X 25 TO IS 1364 PART 2 2002 MATL IS 1367 P14 Gr A2 70 ISO 3506 79, Gr A2 70, STAINLESS STEEL | 360 | NO |  |  | |
| 10 | RFS5310520 | | CSK HD SCREW M5x20 TO IS:1365-2005, PC-4.8, GLVD. | 1512 | NO |  |  | |
| 11 | RFS7620420 | | RFS7620420,CROSS RECESSED PAN HEAD SCREW M4 X 20 TO IS 7483 1985 MATL ISO 3506 79, Gr A2 70,STAINLESS STEEL | 216 | NO |  |  | |
| 12 | RFS7620620 | | HEX HEAD SCREW M6X20 TO IS:1364-(PART-2)-2002/MATL:ISO:3506-79,Gr-A20-70 ,STAINLESS STEEL. | 288 | NO |  |  | |
| 13 | RFW0920409 | | RFW0920409, SPRING WASHER B4 , RIGHT HAND TO IS 3063 1994 MATL AI SI 304, IS 1367 P 14 84, A2 70, SS | 648 | NO |  |  | |
| 14 | RFW0921022 | | RFW0921022, SPRING WASHER B10, RIGHT HAND TO IS 3063 1994 MATL AI SI 304,STAINLESS STEEL IS 1367 P 14 84, A2 70 | 1584 | NO |  |  | |
| 15 | RFW0960825 | | RFW0960825, SPRING WASHER TYPE HEAVY B8 X 2.5 THK, IS 3063 94, TYPE B, RIGHT HAND MATL AISI 304 IS 1367 P14 Gr A2 70,STAINLESS  STEEL | 936 | NO |  |  | |
| 16 | RFW0971635 | | RFW0971635, SPRING WASHER B16 TO IS 3063 1994, DACROTIZE TO SPEC ASTM F1136 GR 6WITH BLACK TOP COAT | 792 | NO |  |  | |
| 17 | RFW2620408 | | RFW2620408, MACHINED WASHER FOR M4 BOLT TO IS 2016 TAB 1 1967 MATL AISI 304 IS 1367 P14 Gr A2 70, STAINLESS STEEL | 648 | NO |  |  | |
| **Column (A)** | | | **Column (B)** | | | **Column (C)**  **(say ‘Yes’ OR ‘’No” in this column, as applicable)** | | |
| **1** | | | Are you an Manufacturer of Hardware / Authorised dealers of reputed make of hardware. Kindly confirm the same and attach relevant documents | | |  | | |
| **2** | | | Any history of pending litigations and Risk purchase against previous orders of BEML | | |  | | |

NOTE: State ‘**YES’ / ‘NO’** as applicable in column (C).

\*Bids of firms having any history of pending litigations, default in and Risk purchase against previous orders of BEML which mention otherwise in this bid confirmation are liable for rejection.

**Name and Signature of authorised rep.**

**of Bidding firm with Seal**